HP computers at SEST

Last Update: 1st of October 2001

Mikael Lerner

Chapter 1

HP computers at SEST

1.1 HP Workstations

1.1.1 Overview

The following tables summarises the configurations of HP the computers used at SEST.

1.1.2 Vela

• Basic properties

Model: HP 9000/778 (B132L) OS: HP-UX B.10.20A Processor: 132 MHz PA-risc 1.1e PA7300 Memory: 132 MB Cache: 64 kB ROM: Firmware 2.5, IODC rev. 1 Machine-ID: 2003552897 Address: 00:60:B0:18:63:63 Monitor: HP P1110, 21” (spare: HP A4331D, 19”)

• Hardware configuration:

Primary boot path: 8/16/5.6.0 Alternate boot path: 8/16/5.3.0 Graphics path: graphics(0) — (type 1: 1280x1024, 75 Hz, VESA) (spare: type 12: 1280x1024, 72 Hz) Keyboard path: PS2

• Hardware SCSI–6 Internal disk — 2 GB IBM DORS–32160 SCSI–5 External disk — 8.7 GB IBM DDRS–39130 SCSI–4 External CD–RW — Yamaha CRW4416SX , SE SCSI SCSI–3 External disk — 4 GB Seagate ST15230N , SE SCSI SCSI–2 Internal CD–ROM — Toshiba XM–5401TA SCSI–1 External DAT — HP C1533A, 4 GB DDS , F/W SCSI SCSI–0 Empty

• Interfaces LAN interface (AUI [with BNC adapter] & twisted pair) 2 * Serial RS-232 interface Parallel interface Single-ended SCSI Audio interface (in & out) Keyboard Mouse Monitor (HP 3-row connector)

• I/O cards:

8/16/0 CentIf Built-in parallel interface 8/16/4 asio0 Built-in RS-232 interface 8/16/5 c720 Built-in SCSI 8/16/6 lan2 Built-in LAN 8/16/7 ps2 Built-in keyboard/mouse 8/20/2 asio0 RS-232 interface (#2) 8/20/5 eisa EISA bus adapter

• Disk usage SCSI–6 — 2 GB — whole — — –/2048 MB SCSI–5 — 8.7 GB — LVM — /vg02 (5) — 8/8712 MB SCSI–3 — 4 GB — LVM — /vg05 (5) — 4/4088 MB

• Local file systems

/ HFS 1752 MB /dev/dsk/c0t6d0 automount
/archive VxFS 2048 MB /dev/vg02/lvol1 automount
/aux2 VxFS 4096 MB /dev/vg02/lvol2 automount
/cdscr VxFS 1536 MB /dev/vg02/lvol3 automount
/logs VxFS 512 MB /dev/vg02/lvol4 automount
/alt VxFS 512 MB /dev/vg02/lvol5 automount
/ HFS 1792 MB /dev/vg05/lvol1 (mirror)
/aux2 VxFS 1536 MB /dev/vg05/lvol3 (mirror)
/archive VxFS 256 MB /dev/vg05/lvol4 (mirror)
/logs VxFS 224 MB /dev/vg05/lvol5 (mirror)
/cdscr VxFS 24 MB /dev/vg05/lvol6 (mirror)
/cdrom CDFS /dev/dsk/c0t4d0
/cdrom CDFS /dev/dsk/c0t2d0

• Imported file systems — only for disk copying

/cdscr/mount update disk/aux2 — RW — carina:/aux2
/cdscr/mount update disk/aux2 — RW — volans:/aux2
/cdscr/mount update disk/archive — RW — volans:/archive
/cdscr/mount update disk/cdscr — RW — volans:/cdscr
/cdscr/mount update disk/logs — RW — volans:/logs

• Exported file systems

none

• Swap and dump space

256 MB primary device swap/dump on /dev/dsk/c0t6d0 252 MB primary device swap/dump on /dev/vg05/lvol2 (mirror)

1.1.3 Puppis

• Basic properties

Model: HP 9000/720 OS: HP-UX B.10.20A Processor: 50 MHz PA-risc 1.1a PA7000 Memory: 132 MB ROM: ???

Machine-ID: 2003885826 Address: 08:00:09:95:5E:70 Monitor: HP A1097C, 19”

• Hardware configuration:

Primary boot path: 2/0/1.6.0 Alternate boot path: 2/0/1.5.0 (non-bootable)

• Hardware SCSI–6 Internal disk — 4.3 GB Seagate ST34520N SCSI–5 Empty SCSI–4 External disk — 8.7 GB Seagate ST39173N , SE SCSI SCSI–3 External disk — 4 GB Seagate ST15230N , SE SCSI SCSI–2 External disk — 4 GB Seagate ST15150N , SE SCSI SCSI–1 External DAT — HP 35480A, 2 GB DDS , F/W SCSI SCSI–0 Empty

• Interfaces LAN interface (AUI & BNC) EISA LAN interface (AUI & BNC) 2 * Serial RS-232 interface Single-ended SCSI Audio (single) HIL device Monitor (3 BNCs)

• I/O cards:

2/0/1 c720 Built-in SCSI 2/0/2 lan2 Built-in LAN 2/0/4 asio0 Built-in RS-232 interface 2/0/5 asio0 Built-in RS-232 interface 2/0/6 CentIf Built-in parallel interface 4 eisa EISA adapter 4/0/1 lan2 EISA card HWP1850

• Disk usage SCSI–6 — 4.3 GB — LVM — /vg00 (8) — 368/4340 MB SCSI–4 — 8.7 GB — LVM — /vg01 (4) — 72/8680 MB SCSI–3 — 4 GB — whole — — –/4095 MB SCSI–2 — 4 GB — LVM — /vg02 (1) — 92/4092 MB

• Local file systems

/stand HFS 48 MB /dev/vg00/lvol1 automount
/ VxFS 84 MB /dev/vg00/lvol3 automount
/opt VxFS 1024 MB /dev/vg00/lvol4 automount
/tmp VxFS 128 MB /dev/vg00/lvol5 automount
/backup VxFS 128 MB /dev/vg00/lvol6 automount
/usr VxFS 1024 MB /dev/vg00/lvol7 automount
/var VxFS 1024 MB /dev/vg00/lvol8 automount
/home HFS 4096 MB /dev/dsk/c0t3d0 automount
/app HFS 2048 MB /dev/vg01/lvol1 automount
/vela archive HFS 4000 MB /dev/vg01/lvol3 automount
/aux3 HFS 2048 MB /dev/vg01/lvol4 automount
/scratch VxFS 4000 MB /dev/vg02/lvol1 automount

• Imported file systems

/aux2 — RW — carina:/aux2

• Exported file systems

/home — RW
/aux2 — RW
/scratch — RW

• Swap and dump space 512 MB primary device swap/dump on /dev/vg00/lvol2 512 MB secondary device swap on /dev/vg01/lvol2

1.1.4 Carina

• Basic properties

Model: HP 9000/730 OS: HP-UX B.10.20A Processor: 66 MHz PA-risc 1.1a PA7000 Memory: 96 MB ROM: PDC 2.1, IODC 2.1 Machine-ID: 2007424834 Address: 08:00:09:24:B4:17 Monitor: HP A4033A, 19”

• Hardware configuration:

Primary boot path: 2/0/1.6.0 Alternate boot path: 2/0/1.4.0 (non-bootable)

• Hardware

SCSI–6 Internal disk — 4.3 GB Seagate ST34520N SCSI–5 Internal disk — 1 GB Seagate ST11220N SCSI–4 External disk — 1.8 GB Seagate ST42100 , F/W SCSI SCSI–3 Empty SCSI–2 External disk — 8.7 GB IBM DDRS–39130 , SE SCSI SCSI–1 Empty SCSI–0 External CD–ROM — Toshiba XM–3401TA, F/W SCSI

• Interfaces

LAN interface (AUI & BNC) 2 * Serial RS-232 interface Single-ended SCSI Audio (single) HIL device Monitor (3 BNCs)

• I/O cards:

2/0/1 c720 Built-in SCSI 2/0/2 lan2 Built-in LAN 2/0/4 asio0 Built-in RS-232 interface 2/0/5 asio0 Built-in RS-232 interface 2/0/6 CentIf Built-in parallel interface

• Disk usage

SCSI–6 — 4.3 GB — LVM — /vg00 (8) — 368/4340 MB SCSI–5 — 1 GB — LVM — /vg04 (1) — 4/1004 MB SCSI–4 — 1.8 GB — LVM — /vg03 (1) — 8/1808 MB SCSI–2 — 8.7 GB — LVM — /vg02 (2) — 520/8712 MB

• Local file systems

/stand HFS 48 MB /dev/vg00/lvol1 automount
/ VxFS 84 MB /dev/vg00/lvol3 automount
/home VxFS 128 MB /dev/vg00/lvol4 automount
/opt VxFS 1024 MB /dev/vg00/lvol5 automount
/tmp VxFS 128 MB /dev/vg00/lvol6 automount
/usr VxFS 1024 MB /dev/vg00/lvol7 automount
/var VxFS 1024 MB /dev/vg00/lvol8 automount
/aux2 VxFS 4096 MB /dev/vg02/lvol1 automount
/staff VxFS 4096 MB /dev/vg02/lvol2 automount
/logs VxFS 1800 MB /dev/vg03/lvol1 automount
/syslogs VxFS 1000 MB /dev/vg04/lvol1 automount
/cdrom CDFS /dev/dsk/c0t0d0

• Imported file systems

/scratch — RW — puppis:/scratch

• Exported file systems

/aux2 — RW

• Swap and dump space 512 MB primary device swap/dump on /dev/vg00/lvol2

1.1.5 Volans

• Basic properties

Model: HP 9000/735 OS: HP-UX B.10.20A Processor: 99 MHz PA-risc 1.1b PA7100 Memory: 144 MB ROM: PDC 1.1, IODC 1.0 Machine-ID: 2014895682 Address: 08:00:09:24:A4:3E Monitor: HP A2094A, 19” (spare: HP A1097C, 19”)

• Hardware configuration:

Primary boot path: 2/0/7.6.0 Alternate boot path: 2/0/1.5.0 (non-existent)

• Hardware

Fast/Wide SCSI chain (2/0/7):

SCSI–6 Internal disk — 4.3 GB Seagate ST34501W SCSI–5 Internal disk — 4.3 GB Seagate ST34501W SCSI–4 Empty SCSI–3 Empty SCSI–2 Empty SCSI–1 Empty SCSI–0 Empty Single-ended SCSI chain (2/0/1): SCSI–6 Empty SCSI–5 Empty SCSI–4 Empty SCSI–3 Empty SCSI–2 External CD–ROM — Toshiba XM–3301TA, F/W SCSI SCSI–1 Empty SCSI–0 Empty

• Interfaces

LAN interface (AUI [with BNC adapter]) 2 * Serial RS-232 interface Parallel interface Single-ended SCSI Fast/Wide SCSI Audio interface (in & out & mic & phones & speakers) HIL device 2 * Monitor (3 BNCs)

• I/O cards:

2/0/1 c720 Built-in SCSI 2/0/2 lan2 Built-in LAN 2/0/4 asio0 Built-in RS-232 interface 2/0/5 asio0 Built-in RS-232 interface 2/0/6 CentIf Built-in parallel interface 2/0/7 c720 Built-in Fast/Wide SCSI 4 eisa EISA adapter

• Disk usage

SCSI–6 — 4.3 GB — LVM — /vg00 (8) — 0/4336 MB SCSI–5 — 4.3 GB — LVM — /vg02 (4) — 240/4336 MB

• Local file systems

/stand HFS 64 MB /dev/vg00/lvol1 automount
/ HFS 96 MB /dev/vg00/lvol3 automount
/home HFS 512 MB /dev/vg00/lvol4 automount
/opt HFS 1024 MB /dev/vg00/lvol5 automount
/tmp HFS 256 MB /dev/vg00/lvol6 automount
/usr HFS 848 MB /dev/vg00/lvol7 automount
/var HFS 1024 MB /dev/vg00/lvol8 automount
/aux2 VxFS 2048 MB /dev/vg02/lvol1 automount
/archive VxFS 512 MB /dev/vg02/lvol2 automount
/cdscr VxFS 1024 MB /dev/vg02/lvol3 automount
/logs VxFS 512 MB /dev/vg02/lvol4 automount
/cdrom CDFS /dev/dsk/c0t2d0

• Imported file systems none

• Exported file systems

/aux2 — RW
/archive — RW
/cdscr — RW
/logs — RW

• Swap and dump space 512 MB primary device swap/dump on /dev/vg00/lvol2