Onsala Clock

The Onsala Clock is not used anymore to produce the 1 PPS signals to the system, the SEST Clock unit does that. BUT the Onsala Clock is used to send a synch signal to both the chopper and the bolometer so it is vital that it is up and running.

To restart the clock:

Open the front panel (two screws at the top) and set the clock ahead of the time shown by the TAC. Then press and and later release the load button at the second before the times matches. Note: This is critical as the Onsala clock is used as a frequency standard for both the chopper wheel and the bolometer.