How to restart the sub-reflector control software

These are the steps to reboot the sub-reflector:

1. Try to move the subreflector with Sub . If the actual positions do not change, it may be a communication problem on the TCS side. Hit Ctrl-c in the TCS window and then type StopTCS followed by StartTCS and display. Try again with Sub . If the problem persists, continue with the following steps.

2. Click on Shell and select Location: Iccabin and click on Accept. It is also possible to open a local shell on VELA and telnet to iccabin (telnet iccabin).

3. login with user michel and the michel password 4. type: subinit 3 5. wait for about 2 minutes for the subreflector to be initialized (this can be seen when the 4 offsets in the TCS windows display of the subreflector offsets no longer are moving).

6. Check that the actual positions are close to the commanded positions of the 4 offsets (within 0.01 for the first two values and within 2.00 for the last two).

7. if this doesn’t work go back and try step 3 and 4 again. 8. If step 6 didn’t solve the problem try:

subinit all

9. wait for 2 minutes (see step 4) 10. exit If this doesn’t solve your problem try doing the steps in section ⁀”How to reset ICCABIN and ANTLIA”