Subreflector is not tracking

If the subreflector does not seem to move (e.g. during a subpointing routine), if you get uncommonly high errors, or, if the source is not seen, then the subreflector may not be tracking properly or may be stuck in one of the initialization positions. In this case the subreflector has to be reinitialized. See section "How to restart the sub-reflector control software" on how this can be solved easily and quickly without running off up to the antenna.