Possible TCS Problems

TCS misbehaviour might appear with different degrees of severity. Sometimes it simply seems to hang. A very diagnostic way to verify this, is to see if the numbers on the TCS display are updated. In a few cases, this especially was true for the subreflector settings. This comparably slight problem typically originates from communication breakdowns or the crash of processes. Sometimes the pointing seems to drift away slowly when the TCS has been a long time without a reboot. So, if you suspect that this has happened, you might want to restart the TCS according to the steps described in Section ⁀”TCS Replacement”.