How to reset ICCABIN and ANTLIA

1. Click on Shell and select Location: Iccabin and click on Accept. It is also possible to open a local shell on VELA and telnet to iccabin (telnet iccabin).

2. login with user michel and the michel password 3. type reset 4. wait at least 40 seconds 5. In the TCS display window hit Ctrl-c. If you don’t have a TCS window open follow the steps below:

(a) Click on Shell and select Location: Antlia and click on Accept. It is also possible to open a local shell on VELA and telnet to antlia (telnet antlia).

(b) login with user tcs and the guest password 6. type StopTCS followed by StopTCS and display 7. The subreflector should be initialised by now. Check that the actual position agrees with the commanded position.

Sometimes the culprit is NOT ICCABIN or ANTLIA but ICCNTRL. Symptoms of a problem with ICCNTRL is that Connect and Quasi are not responding and the steps above didn’t solve the solution. In this case try the solution in section ⁀”Rebooting ICCNTRL VME rack”. Note: You can always do a hard reboot instead of using the reset command via telnet but this should be only used as a last solution. A hard reboot is when the power is cycled on and off on the pertinent machine. See Section ⁀”Rebooting the Cabin Controller VME” for a description of a full hardware reboot of ICCABIN.