Rebooting VELA

Note: Before fiddling with VELA talk to the system manager or if he isn’t available then read the pertinent sections in SEST System Administration Handbook. This section here is a short description of the procedures and if you are unfamiliar with these proceedings then it is important to check the Handbook.

Never turn off VELA’s power switch while the system is up. This can corrupt the file system and in the worst case the machine may not start up again. In the case the system is behaving well, but you want to reboot the machine for whatever reason, do as follows:

• Exit the user session • log in as daprog or as director • open a terminal window ( Shell and selecting local and clicking on Accept) • type: cd / • type: /sbin/shutdown -ry 0 and wait several minutes until VELA is rebooted.

The machine will be ready when the login screen appears again.

In case VELA refuses a login to any user by saying that the login sessions have been locked, you only need to restart the login screen of the HPVUE manager from the Options menu. In case VELA really hangs, and there is no way to login, do as follows:

• use an X-terminal and login to PUPPIS using the account of your choice • open a terminal window on PUPPIS • type: telnet vela • log in as daprog • type: cd / • type: /sbin/shutdown -ry 0 and wait several minutes until vela is rebooted.

The machine will be ready when the login screen appears again.